**Cleaning and Care Maintenance for Powder Coated Material**

Below is a suggested method of cleaning and care for JAG Metal Solutions, Inc. powder coated products.

Select a cleaning solution that is safe to contact with the bare hands. Solutions should be mild, such as a product used to wash a vehicle. Please steer clear from using any acidic solutions. Such solutions may damage the finish of the powder coat leading to discoloration.

Use a soft cloth, such as microfiber, to clean the surface of the product. Do not use abrasive materials on the product. Such materials may scratch and damage the powder coat finish.

Rinse the surface thoroughly with clean water and the selected mild soap, and then dry the surface with a clean soft cloth. Repeat until dirt is removed and surface is clean.

In areas were the product is exposed to heavy pollutants or salt spray, such as but not limited to coastal areas, cleaning should take place on a minimum once per month basis. Cleaning and maintenance should be part of a regular maintenance program.